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Absolute Maximum Ratings (Ta = 25 °C)

Characteristics Symbol Rating Unit
Output voltage Vour 50 v
COMMON pin voltage Vo 051050 v
Output current Tout 500 mAJch
Input voltage Vin 05030 v
Clamp diode reverse voltage |V 50 v
Clamp diode forward current IF 500 mA
PG (Note1) 147
Power FG (Note2) . 0.96 w
dissipation TENG (Note3) o 0.96
FWG (Noted) 131
Operating temperature Toor 401085 °C
Storage temperature Too 550 150 °C
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Electrical Characteristics (Ta = 25°C unless otherwise noted)

Characteristics symbol | et Condition Min | Typ. | Max | Unit
Output leakage current | lieak 1 xc'" 03""‘ Ta=85C — | = | 10| w
'
R - _ |07 114
lour = 350 A, Vi =5.0V o0 | @26
TBD62083A - - 04 | 065
De208 lour =200 mA,Viy =50V | — | 04| 39
Output
- - _ | 02 [o32s
voltage Vos lour = 100 mA, Vi =5.0V 20) |G25)|
(Output Row | 2 )
ON-resistan lour =350 mA, Viy=7.0v | — | 07 | 114
) (20) | (3.25)
TBD62084A - - _ | 04 |oes
Dg208 lour = 200 mA, Vi =7.0V 50 a5
- - _ | 02 [o32s
lour = 100 mA, Vi =7.0V o |2
TBD62083A - _ | —
Input Do20s Vin=25V 0.1
current Inow |3 mA
(Output on) | TBD62084A Vin=7.0V — | — |os
series
Input current(Output off) [Inorr)| 4 [Vn=0V,Ta=85C - — 10 | wA
put | TED020834 _ 228
In| series B
voltage Vinowm| 5 |lour=100mA, Vour=2V v
(Output on) | TBD62084A — — | 70
series
Clamp diode _ . N
o ) 6 [ve=50V,Ta=85°C 10 | wA
Clamp diode _ — | _
fooman votoge Ve 7 [le=350mA 20 [ v
Tum-on delay ton Vour =50 V — (o4 | —
8 [R=1250 s
Tum-off delay torr 5 oF — Jos | —





