
協作型6軸機器手臂兩套內含
項目1( x2set)ABB POWA CRB1810-10/1.526軸手臂( 荷重10公斤，最大工作半徑1.52M)
項目2(x2set)控制系統包含控制箱OmnicoreE10及彩色觸控螢幕之教導盒
項目3(x2set ) 控制箱及彩色觸控螢幕之教導盒皆可透過其USB傳輸程式及儲存檔案
項目4(x2set ) I/O(輸入/輸出)配置8IN/6OUT數位對外部控制訊號
項目5(x2set ) ABB POWA CRB1810-10/1.52
項目6搬運吊裝及定位安裝
保固一年
ABB POWA CRB1810依下表規格附ABB出廠檢測資料
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OmnicoreE10控制系統包含控制箱及教導盒
[image: The image depicts a sleek, modern device with the ABB OmniCore E10 branding, showcasing an interface and a clear, professional setting.

AI 產生的內容可能不正確。]
[image: The Omnicore E10 controller is a robust industrial device featuring PROFINET and Ethernet/IP communication protocols, an 8

AI 產生的內容可能不正確。]

控制系統 Omnicore 控制器
[image: The image shows a person using a computer-controlled CNC milling machine, with a hand-operated control panel and a 3D model displayed on the screen.

AI 產生的內容可能不正確。]
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TRAINING
OmniCore™
E1O Type A Walkthrough
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Bimensions (Wx D x ) 45 % 340 x Bomm

weight 12 kg

1P Level P20

Avellebia EomGAICR S PlalaEawes PROFINET Controller, PROFINET Device, PROFisafe

Controller, PROFIsafe Device, CC-Link IE MASTER, CC- Link
IE Device, CC — Link Safety Master==, CC ~ Link Safoty
Devicar+, EtherCAT device, EtherCAT Master-+, EtherCAT
FSOE device, EtherCAT FSoE Master-+, Etharnet/IP
Adapter, Ethernet/IP Scanner, CIP Safety Adapter-, CIP
Safety Scanner-+ = Coming soon

interface Built In16D1/8D0

Cable length to Flexpendant sm

Flexpendant

Screen T color touch screen
Resotution 1024x768
Protection Pes.

waeight 1.2kg
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