五軸體積空間精度補償系統之操作面板與鍵盤
一.工作項目：

1.預防斷電功能USB標準鍵盤電路板設計與製作

2.EtherCAT_4832IO機械操作面板與電路板製作

二.工作規範：

1.預防斷電功能USB標準鍵盤電路板設計與製作
a.尺寸介面如圖一

b.面板所需功能需求分鍵盤功能及操作面板功能,細部功能說明請參考圖二、圖三、圖四
c.需依設計USB擴充模組
d.需設計標準鍵盤USB界面之解碼電路電路板
e.需搭配後蓋板板金設計
f.需提供所需之各式按鍵
g.需提按鍵雷射雕刻印圖案及固定鐵板當前板
h.需預留前方延伸擴充USB插座一組及防塵蓋
i.提供2米長USB延長連接電纜線

j.按鍵需設計具有防水防塵功能
k.需提供三組作樣品
l.需具備作業系統關機啟動功能
2. EtherCAT_4832IO卡操作面板設計與電路板設計與製作
a.需搭配EtherCAT_4832 IO卡之尺寸固定

b.需提供波段開關及緊急停止開關

c.需提供所需之各式按鍵
d.需提供按鍵雷射雕刻印圖案及固定鐵板當前板
e.需提供EtherCAT_4832 IO卡之全包覆後蓋板板金設計
f.按鍵需設計具有防水防塵功能

g.面板輸出及輸入點規劃如附件表1
h.需提供三組作樣品

i.需製作電路板電路設計及電路板印刷電路設計

j.電源開關、程式執行與暫停按鈕以可更換式按鈕型式設定

k.電源關、程式暫停鈕需有保護蓋

l.需依照EtherCAT_4832 IO卡之接腳位址定義設計ladder
b.設計ladder需可提供M100控制器使用
c.需提供ladder工作專案檔
d.需熟悉M100控制器操作與使用
三.附件：

圖一
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圖二
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圖三
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圖四
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表1
輸入點
	位址
	
	48/32說明

	I0
	
	+X PB

	I1
	
	-X PB

	I2
	
	+Y PB

	I3
	
	-Y PB

	I4
	
	+Z PB

	I5
	
	-Z PB

	I6
	
	+4 PB

	I7
	
	-4 PB

	I8
	
	+5 PB

	I9
	
	-5 PB

	I10
	
	Spindle CW PB

	I11
	
	Spindle CCW PB

	I12
	
	ORCM PB

	I13
	
	ATC CW PB

	I14
	
	ATC CCW PB

	I15
	
	Coolant manual PB

	I16
	
	Work lamp PB

	I17
	
	DOOR PB

	I18
	
	RESET PB/SP STOP

	I19
	
	Screw CW PB

	I20
	
	Screw CCW PB

	I21
	
	Cycle start PB

	I22
	
	Feed hold PB

	I23
	
	Feedrate bit 1

	I24
	
	Feedrate bit 2

	I25
	
	Feedrate bit 4

	I26
	
	Feedrate bit 8

	I27
	
	Feedrate bit 16

	I28
	
	Rotate SW inhibit

	I29
	
	MPG *1 mode PB

	I30
	
	MPG-*10

	I31
	
	MPG-*100

	I32
	
	JOG mode PB

	I33
	
	RAPID mode PB

	I34
	
	HOME mode  PB

	I35
	
	MEMORY mode PB

	I36
	
	MDI mode PB

	I37
	
	EDIT mode PB

	I38
	
	RAPID override – PB

	I39
	
	RAPID override 100 PB

	I40
	
	RAPID override + PB

	I41
	
	SP override – PB

	I42
	
	SP override 100 PB

	I43
	
	SP override + PB

	I44
	
	MPG-AXIS bit 0

	I45
	
	MPG-AXIS bit 1

	I46
	
	MPG-AXIS bit 2

	I47
	
	MPG ESP


輸出點
	位址
	48/32說明

	O0
	X1 LED

	O1
	Y1 LED

	O2
	Z1 LED

	O3
	41 LED

	O4
	51 LED

	O5
	Spin CW LED

	O6
	Spin CCW LED

	O7
	ORCM LED

	O8
	ATC CW LED

	O9
	ATC CCW LED

	O10
	Coolant manual LED

	O11
	Work lamp LED

	O12
	DOOR LED

	O13
	Reset LED

	O14
	Screw CW LED

	O15
	Screw CCW LED

	O16
	OT. LED

	O17
	Cycle start LED

	O18
	Feed hold LED

	O19
	MPG *1 MODE LED

	O20
	MPG *10 MODE LED

	O21
	MPG *100 MODE LED

	O22
	JOG MODE LED

	O23
	RAPID MODE LED

	O24
	HOME MODE LED

	O25
	MEMORY MODE LED

	O26
	MDI MODE LED

	O27
	EDIT MODE LED

	O28
	RAPID OVER. 100% LED

	O29
	SP OVER. 100% LED

	O30
	MPG MODE LAMP

	O31
	蜂鳴器


七 驗收標準
1.外觀
[image: image5.emf]
2.樣品數量:3組
3.2米長USB連接電纜線:3條
4.ladder專案檔:1案

5.USB模組專用電源供應器:3組

6.作業系統關機啟動功能
