規格要求:
1. 生命週期評估（LCA）的第一階段，涵蓋製造程序之環境/碳影響的「廠內階段（Gate-to-Gate）」評估。

	
		Life Cycle Assessment (LCA) 




	Standard
		ISO 14040 / ISO 14044 




	Methodology
		EU Environmental Footprint EF3.1 




	Scope
		Multiple environmental impact categories 




	Best for
		EU market compliance, full environmental impact picture 






2. 必須涵蓋下列程序:
Kick-off 
1) define the scope, functional unit and first assumptions aligned to ISO 14067 (PCF) or ISO 14044 (LCA). Data requirements are highlighted and the full process is outlined in detail.
Data collection 
1) Positive Planet provides data collection forms. Regular touch points support your team through the process. Missing or upstream data (Phase 2) is handled through agreed assumptions and background data collection by Positive Planet.
Modelling 
1) Processes as defined in the goal and scope are modelled, primary data is implemented, and any sensitivity and scenario analysis agreed in the scope definition is included.
Impact assessment (LCIA) 
1) Climate change impact potential is calculated using dedicated LCA software and Ecoinvent emission factors. IPCC AR6 methodology for PCF; EU EF3.1 for LCA. Sensitivity and scenario analysis covers manufacturing uncertainties and decarbonisation opportunities.
Reporting 
1) A comprehensive LCA report is provided covering Goal & Scope, LCI, LCIA and Interpretation, structured to comply with the relevant ISO standard. Executive summary slides are also included for internal dissemination.

